 Product Description Fortinet FortiAP 221E - wireless access point

 Device Type Wireless access point

 Form Factor External - indoor

 Data Link Protocol IEEE 802.11b, IEEE 802.11a, IEEE 802.11g, IEEE 802.11n, IEEE 802.11ac Wave 2

 Frequency Band 2.4 GHz, 5 GHz

 Performance Maximum throughput (2.4 GHz): 300 Mbps ¦ Maximum throughput (5 GHz): 867 Mbps

 Capacity Maximum number of configured SSIDs: 16 ¦ Concurrent users per radio: 512

 Included Accessories Wall mounting kit, ceiling mounting kit, T-Rail mounting kit

 Power Over Ethernet (PoE) Supported PoE

 Power AC 120/230 V (50/60 Hz)

 Dimensions (WxDxH) 6.3 in x 6.3 in x 1.9 in

 Weight 17.64 oz